

|  |
| --- |
| STATIC CONCRETE PUMPSwww.ramcrete.co.uk01628 782 860 |



 **Technical data Cifa P506 / 309**

|  |  |
| --- | --- |
| **Delivery Cylinder**  | **176mm** |
| **Delivery Stroke** | **1000mm** |
| **Output** |  **Max \*52m3/hr / ^34m3/hr** |
| **Delivery pressure**  | **\*57 Bar / ^ 91 Bar** |
| **Strokes per minute** | **\*36 / ^ 24** |
| **Engine Power** | **72kw** |
| **Weight** | **3400kg** |
| **Pressure connection**  | **5 inch** |

**\* Rod side ^ Piston side**

**Generic Length 4315mm , Width 1570mm , Height 2175mm**